From 54ca11a48eba11788445247b16bc77637e3aa84a Mon Sep 17 00:00:00 2001
From: Jan Beulich <jbeulich@suse.com>
Date: Thu, 22 Jul 2021 13:07:27 +0200
Subject: [PATCH] x86: correct EVEX.V' handling outside of 64-bit mode

Unlike the high bit of VEX.vvvv / EVEX.vvvv, EVEX.V' is not ignored
outside of 64-bit mode. Oddly enough there already are tests for these
cases, but their expectations were wrong. (This may have been based on
an old SDM version, where the restriction wasn't properly spelled out.)

diff --git a/gas/testsuite/gas/i386/noextreg.d b/gas/testsuite/gas/i386/noextreg.d
index 08bad494a80..ba175fc001e 100644
--- a/gas/testsuite/gas/i386/noextreg.d
+++ b/gas/testsuite/gas/i386/noextreg.d
@@ -13,14 +13,14 @@ Disassembly of section .text:
 [ 	]*[a-f0-9]+:	62 f1 7d 08 db c0    	vpandd %xmm0,%xmm0,%xmm0
 [ 	]*[a-f0-9]+:	62 d1 7d 08 db c0    	vpandd %xmm0,%xmm0,%xmm0
 [ 	]*[a-f0-9]+:	62 f1 3d 08 db c0    	vpandd %xmm0,%xmm0,%xmm0
-[ 	]*[a-f0-9]+:	62 f1 7d 00 db c0    	vpandd %xmm0,%xmm0,%xmm0
+[ 	]*[a-f0-9]+:	62 f1 7d 00 db c0    	vpandd %xmm0,\(bad\),%xmm0
 [ 	]*[a-f0-9]+:	c4 e3 79 4c c0 00    	vpblendvb %xmm0,%xmm0,%xmm0,%xmm0
 [ 	]*[a-f0-9]+:	c4 c3 79 4c c0 00    	vpblendvb %xmm0,%xmm0,%xmm0,%xmm0
 [ 	]*[a-f0-9]+:	c4 e3 39 4c c0 00    	vpblendvb %xmm0,%xmm0,%xmm0,%xmm0
 [ 	]*[a-f0-9]+:	c4 e3 79 4c c0 80    	vpblendvb %xmm0,%xmm0,%xmm0,%xmm0
 [ 	]*[a-f0-9]+:	62 f2 7d 0f 90 0c 00 	vpgatherdd \(%eax,%xmm0,1\),%xmm1\{%k7\}
 [ 	]*[a-f0-9]+:	62 d2 7d 0f 90 0c 00 	vpgatherdd \(%eax,%xmm0,1\),%xmm1\{%k7\}
-[ 	]*[a-f0-9]+:	62 f2 7d 07 90 0c 00 	vpgatherdd \(%eax,%xmm0,1\),%xmm1\{%k7\}
+[ 	]*[a-f0-9]+:	62 f2 7d 07 90 0c 00 	vpgatherdd \(%eax,\(bad\),1\),%xmm1\{%k7\}
 [ 	]*[a-f0-9]+:	c4 e2 78 f2 00       	andn   \(%eax\),%eax,%eax
 [ 	]*[a-f0-9]+:	c4 e2 38 f2 00       	andn   \(%eax\),%eax,%eax
 [ 	]*[a-f0-9]+:	c4 c2 78 f2 00       	andn   \(%eax\),%eax,%eax
diff --git a/opcodes/i386-dis.c b/opcodes/i386-dis.c
index ddb659fb041..267d58d535e 100644
--- a/opcodes/i386-dis.c
+++ b/opcodes/i386-dis.c
@@ -9316,7 +9316,6 @@ get_valid_dis386 (const struct dis386 *dp, disassemble_info *info)
 	  /* In 16/32-bit mode silently ignore following bits.  */
 	  rex &= ~REX_B;
 	  vex.r = 1;
-	  vex.v = 1;
 	}
 
       need_vex = 1;
@@ -11718,8 +11717,13 @@ OP_E_memory (int bytemode, int sizeflag)
 		      *obufp = '\0';
 		    }
 		  if (haveindex)
-		    oappend (address_mode == mode_64bit && !addr32flag
-			     ? indexes64[vindex] : indexes32[vindex]);
+		    {
+		      if (address_mode == mode_64bit || vindex < 16)
+			oappend (address_mode == mode_64bit && !addr32flag
+				 ? indexes64[vindex] : indexes32[vindex]);
+		      else
+			oappend ("(bad)");
+		    }
 		  else
 		    oappend (address_mode == mode_64bit && !addr32flag
 			     ? index64 : index32);
@@ -13256,7 +13260,15 @@ OP_VEX (int bytemode, int sizeflag ATTRIBUTE_UNUSED)
   reg = vex.register_specifier;
   vex.register_specifier = 0;
   if (address_mode != mode_64bit)
-    reg &= 7;
+    {
+      if (vex.evex && !vex.v)
+	{
+	  oappend ("(bad)");
+	  return;
+	}
+
+      reg &= 7;
+    }
   else if (vex.evex && !vex.v)
     reg += 16;
 
-- 
2.33.0

