From 5af68a4b3406c0477a2a0c33c546795d6be7f6a5 Mon Sep 17 00:00:00 2001
From: Huisong Li <lihuisong@huawei.com>
Date: Mon, 19 Dec 2022 15:06:44 +0800
Subject: cryptodev: fix telemetry data truncation
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

[ upstream commit 45038f04ab577db8844ef54d7f523119be6c205f ]

The 'u32' data can not assigned to 'int' type variable. The 'u32' data
needs to use the 'u64' APIs to add.

Fixes: d3d98f5ce9d0 ("cryptodev: support telemetry")
Cc: stable@dpdk.org

Signed-off-by: Huisong Li <lihuisong@huawei.com>
Acked-by: Morten Brørup <mb@smartsharesystems.com>
Acked-by: Chengwen Feng <fengchengwen@huawei.com>
---
 lib/cryptodev/rte_cryptodev.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/lib/cryptodev/rte_cryptodev.c b/lib/cryptodev/rte_cryptodev.c
index a40536c5ea..23e079d639 100644
--- a/lib/cryptodev/rte_cryptodev.c
+++ b/lib/cryptodev/rte_cryptodev.c
@@ -2472,7 +2472,7 @@ cryptodev_handle_dev_info(const char *cmd __rte_unused,
 	rte_tel_data_start_dict(d);
 	rte_tel_data_add_dict_string(d, "device_name",
 		cryptodev_info.device->name);
-	rte_tel_data_add_dict_int(d, "max_nb_queue_pairs",
+	rte_tel_data_add_dict_u64(d, "max_nb_queue_pairs",
 		cryptodev_info.max_nb_queue_pairs);
 
 	return 0;
-- 
2.23.0

