From 1f69ffe589f7225a1db83377e276ddbab963bd16 Mon Sep 17 00:00:00 2001
From: jikai <jikai11@huawei.com>
Date: Tue, 21 May 2024 01:13:08 +0000
Subject: [PATCH 091/108] add enable cri v1 in k8s integration

Signed-off-by: jikai <jikai11@huawei.com>
---
 docs/manual/k8s_integration.md    | 9 +++++++++
 docs/manual/k8s_integration_zh.md | 9 +++++++++
 2 files changed, 18 insertions(+)

diff --git a/docs/manual/k8s_integration.md b/docs/manual/k8s_integration.md
index 8fcd0a54..14de0ef4 100644
--- a/docs/manual/k8s_integration.md
+++ b/docs/manual/k8s_integration.md
@@ -20,6 +20,15 @@
 
    if `hosts` is not configured, the default endpoint is `unix:///var/run/isulad.sock`.
 
+   `iSulad` supports both `CRI V1alpha2` and `CRI V1`, and uses `CRI V1alph2` by default.
+   If `CRI V1` is required, it can be configured in `/etc/isulad/daemon.json` to enable `CRI V1`:
+
+   ```json
+       "enable-cri-v1": true,
+   ```
+
+   If `iSulad` is compiled from source codes, `-D ENABLE_CRI_API_V1=ON` option is required in cmake.
+
 2. Restart `isulad`:
 
    ```bash
diff --git a/docs/manual/k8s_integration_zh.md b/docs/manual/k8s_integration_zh.md
index 6dda1e4d..26ba6cc4 100644
--- a/docs/manual/k8s_integration_zh.md
+++ b/docs/manual/k8s_integration_zh.md
@@ -20,6 +20,15 @@
 
    如果`hosts`没有配置，默认的`endpoint`为``unix:///var/run/isulad.sock``
 
+   `iSulad`同时支持`CRI V1alpha2`和`CRI V1`两种`CRI`接口，默认使用`CRI V1alph2`，若需使用`CRI V1`，
+   需要在`/etc/isulad/daemon.json`对`iSulad`进行相关配置，配置方式为：
+
+   ```json
+       "enable-cri-v1": true,
+   ```
+
+   若使用源码编译`iSulad`，还需在编译时增加cmake编译选项`-D ENABLE_CRI_API_V1=ON`。
+
 2. 重启`isulad`
 
    ```bash
-- 
2.25.1

