From 11d8e9f6d54a606163a452f1c8beaa5bc90e949c Mon Sep 17 00:00:00 2001
From: jiangheng <jiangheng14@huawei.com>
Date: Wed, 28 Dec 2022 21:25:36 +0800
Subject: [PATCH] listen pcb also use pcb_if

---
 src/include/lwip/ip.h  | 1 +
 src/include/lwip/tcp.h | 1 -
 2 files changed, 1 insertion(+), 1 deletion(-)

diff --git a/src/include/lwip/ip.h b/src/include/lwip/ip.h
index d560f6b..4cf5f5e 100644
--- a/src/include/lwip/ip.h
+++ b/src/include/lwip/ip.h
@@ -79,6 +79,7 @@ extern "C" {
   ip_addr_t remote_ip;                     \
   /* Bound netif index */                  \
   u8_t netif_idx;                          \
+  struct netif *pcb_if;                     \
   /* Socket options */                     \
   u8_t so_options;                         \
   /* Type Of Service */                    \
diff --git a/src/include/lwip/tcp.h b/src/include/lwip/tcp.h
index 97cb882..0b65b01 100644
--- a/src/include/lwip/tcp.h
+++ b/src/include/lwip/tcp.h
@@ -409,7 +409,6 @@ struct tcp_pcb {
   u8_t snd_scale;
   u8_t rcv_scale;
 #endif
-  struct netif* pcb_if;
 };

 #if TCP_PCB_HASH
--
2.23.0

