From 74ef18c90684f0ae18aef071b9e11a5e8796177b Mon Sep 17 00:00:00 2001
From: alexchen <alex.chen@huawei.com>
Date: Tue, 8 Sep 2020 11:17:20 +0000
Subject: [PATCH] hw/block/nvme: fix pin-based interrupt behavior

First, since the device only supports MSI-X or pin-based interrupt, if
MSI-X is not enabled, it should not accept interrupt vectors different
from 0 when creating completion queues.

Secondly, the irq_status NvmeCtrl member is meant to be compared to the
INTMS register, so it should only be 32 bits wide. And it is really only
useful when used with multi-message MSI.

Third, since we do not force a 1-to-1 correspondence between cqid and
interrupt vector, the irq_status register should not have bits set
according to cqid, but according to the associated interrupt vector.

Fix these issues, but keep irq_status available so we can easily support
multi-message MSI down the line.

Fixes: 5e9aa92eb1a5 ("hw/block: Fix pin-based interrupt behaviour of NVMe")
Cc: "Michael S. Tsirkin" <mst@redhat.com>
Cc: Marcel Apfelbaum <marcel.apfelbaum@gmail.com>
Signed-off-by: Klaus Jensen <k.jensen@samsung.com>
Reviewed-by: Keith Busch <kbusch@kernel.org>
Message-Id: <20200609190333.59390-8-its@irrelevant.dk>
Signed-off-by: Kevin Wolf <kwolf@redhat.com>
Signed-off-by: BiaoXiang Ye <yebiaoxiang@huawei.com>
Signed-off-by: Zhenyu Ye <yezhenyu2@huawei.com>
---
 hw/block/nvme.c | 12 ++++++++----
 hw/block/nvme.h |  2 +-
 2 files changed, 9 insertions(+), 5 deletions(-)

diff --git a/hw/block/nvme.c b/hw/block/nvme.c
index 36d6a8bb..e35c2e10 100644
--- a/hw/block/nvme.c
+++ b/hw/block/nvme.c
@@ -115,8 +115,8 @@ static void nvme_irq_assert(NvmeCtrl *n, NvmeCQueue *cq)
             msix_notify(&(n->parent_obj), cq->vector);
         } else {
             trace_nvme_irq_pin();
-            assert(cq->cqid < 64);
-            n->irq_status |= 1 << cq->cqid;
+            assert(cq->vector < 32);
+            n->irq_status |= 1 << cq->vector;
             nvme_irq_check(n);
         }
     } else {
@@ -130,8 +130,8 @@ static void nvme_irq_deassert(NvmeCtrl *n, NvmeCQueue *cq)
         if (msix_enabled(&(n->parent_obj))) {
             return;
         } else {
-            assert(cq->cqid < 64);
-            n->irq_status &= ~(1 << cq->cqid);
+            assert(cq->vector < 32);
+            n->irq_status &= ~(1 << cq->vector);
             nvme_irq_check(n);
         }
     }
@@ -630,6 +630,10 @@ static uint16_t nvme_create_cq(NvmeCtrl *n, NvmeCmd *cmd)
         trace_nvme_err_invalid_create_cq_addr(prp1);
         return NVME_INVALID_FIELD | NVME_DNR;
     }
+    if (unlikely(!msix_enabled(&n->parent_obj) && vector)) {
+        trace_nvme_err_invalid_create_cq_vector(vector);
+        return NVME_INVALID_IRQ_VECTOR | NVME_DNR;
+    }
     if (unlikely(vector > n->num_queues)) {
         trace_nvme_err_invalid_create_cq_vector(vector);
         return NVME_INVALID_IRQ_VECTOR | NVME_DNR;
diff --git a/hw/block/nvme.h b/hw/block/nvme.h
index 557194ee..f4c1ff91 100644
--- a/hw/block/nvme.h
+++ b/hw/block/nvme.h
@@ -78,7 +78,7 @@ typedef struct NvmeCtrl {
     uint32_t    cmbsz;
     uint32_t    cmbloc;
     uint8_t     *cmbuf;
-    uint64_t    irq_status;
+    uint32_t    irq_status;
     uint64_t    host_timestamp;                 /* Timestamp sent by the host */
     uint64_t    timestamp_set_qemu_clock_ms;    /* QEMU clock time */
 
-- 
2.23.0

