From 4050da82f772478e1ebbcc6bd1971ecfa07399ad Mon Sep 17 00:00:00 2001
From: Guofeng Yue <yueguofeng@hisilicon.com>
Date: Mon, 17 Oct 2022 11:12:15 +0800
Subject: Update kernel headers

To commit ?? ("RDMA/hns: Pass mac type to user driver for RoH mode").

Signed-off-by: Guofeng Yue <yueguofeng@hisilicon.com>
---
 kernel-headers/rdma/hns-abi.h | 2 ++
 1 file changed, 2 insertions(+)

diff --git a/kernel-headers/rdma/hns-abi.h b/kernel-headers/rdma/hns-abi.h
index 542be5e..9866c51 100644
--- a/kernel-headers/rdma/hns-abi.h
+++ b/kernel-headers/rdma/hns-abi.h
@@ -116,6 +116,8 @@ struct hns_roce_ib_alloc_ucontext_resp {
 	__u32	reserved;
 	__u32   config;
 	__u32   max_inline_data;
+	__u8    mac_type;
+	__u8    rsv1[7];
 };
 
 struct hns_roce_ib_alloc_ucontext {
-- 
2.30.0

