From b88e6ae3e144651092bce923123ca20361cdacab Mon Sep 17 00:00:00 2001
From: Yixing Liu <liuyixing1@huawei.com>
Date: Tue, 27 Sep 2022 19:06:00 +0800
Subject: [PATCH 12/12] libhns: Support DSCP

This patch adds user mode DSCP function through
the mapping of dscp-tc configured in kernel mode.

Signed-off-by: Yixing Liu <liuyixing1@huawei.com>
---
 providers/hns/hns_roce_u.h       |  7 +++++++
 providers/hns/hns_roce_u_abi.h   |  6 ++++++
 providers/hns/hns_roce_u_hw_v2.c | 19 +++++++++++++++----
 providers/hns/hns_roce_u_verbs.c |  7 +++++--
 4 files changed, 33 insertions(+), 6 deletions(-)

diff --git a/providers/hns/hns_roce_u.h b/providers/hns/hns_roce_u.h
index 6b64cd0..8c1cb1e 100644
--- a/providers/hns/hns_roce_u.h
+++ b/providers/hns/hns_roce_u.h
@@ -175,6 +175,11 @@ enum hns_roce_db_type {
 	HNS_ROCE_DB_TYPE_NUM
 };

+enum hns_roce_tc_map_mode {
+	HNS_ROCE_TC_MAP_MODE_PRIO,
+	HNS_ROCE_TC_MAP_MODE_DSCP,
+};
+
 struct hns_roce_db_page {
 	struct hns_roce_db_page	*prev, *next;
 	struct hns_roce_buf	buf;
@@ -315,6 +320,8 @@ struct hns_roce_qp {
 	unsigned int			next_sge;
 	int				port_num;
 	uint8_t				sl;
+	uint8_t				tc_mode;
+	uint8_t				priority;
 	unsigned int			qkey;
 	enum ibv_mtu			path_mtu;

diff --git a/providers/hns/hns_roce_u_abi.h b/providers/hns/hns_roce_u_abi.h
index 2753d30..0519ac7 100644
--- a/providers/hns/hns_roce_u_abi.h
+++ b/providers/hns/hns_roce_u_abi.h
@@ -49,6 +49,9 @@ DECLARE_DRV_CMD(hns_roce_create_cq_ex, IB_USER_VERBS_EX_CMD_CREATE_CQ,
 DECLARE_DRV_CMD(hns_roce_alloc_ucontext, IB_USER_VERBS_CMD_GET_CONTEXT,
 		hns_roce_ib_alloc_ucontext, hns_roce_ib_alloc_ucontext_resp);

+DECLARE_DRV_CMD(hns_roce_create_ah, IB_USER_VERBS_CMD_CREATE_AH, empty,
+		hns_roce_ib_create_ah_resp);
+
 DECLARE_DRV_CMD(hns_roce_create_qp, IB_USER_VERBS_CMD_CREATE_QP,
 		hns_roce_ib_create_qp, hns_roce_ib_create_qp_resp);

@@ -61,4 +64,7 @@ DECLARE_DRV_CMD(hns_roce_create_srq, IB_USER_VERBS_CMD_CREATE_SRQ,
 DECLARE_DRV_CMD(hns_roce_create_srq_ex, IB_USER_VERBS_CMD_CREATE_XSRQ,
 		hns_roce_ib_create_srq, hns_roce_ib_create_srq_resp);

+DECLARE_DRV_CMD(hns_roce_modify_qp_ex, IB_USER_VERBS_EX_CMD_MODIFY_QP,
+		empty, hns_roce_ib_modify_qp_resp);
+
 #endif /* _HNS_ROCE_U_ABI_H */
diff --git a/providers/hns/hns_roce_u_hw_v2.c b/providers/hns/hns_roce_u_hw_v2.c
index a30d461..c652eea 100644
--- a/providers/hns/hns_roce_u_hw_v2.c
+++ b/providers/hns/hns_roce_u_hw_v2.c
@@ -1543,10 +1543,11 @@ static void record_qp_attr(struct ibv_qp *qp, struct ibv_qp_attr *attr,
 static int hns_roce_u_v2_modify_qp(struct ibv_qp *qp, struct ibv_qp_attr *attr,
 				   int attr_mask)
 {
-	int ret;
-	struct ibv_modify_qp cmd;
+	struct hns_roce_modify_qp_ex_resp resp_ex = {};
+	struct hns_roce_modify_qp_ex cmd_ex = {};
 	struct hns_roce_qp *hr_qp = to_hr_qp(qp);
 	bool flag = false; /* modify qp to error */
+	int ret;

 	if ((attr_mask & IBV_QP_STATE) && (attr->qp_state == IBV_QPS_ERR)) {
 		pthread_spin_lock(&hr_qp->sq.lock);
@@ -1554,7 +1555,9 @@ static int hns_roce_u_v2_modify_qp(struct ibv_qp *qp, struct ibv_qp_attr *attr,
 		flag = true;
 	}

-	ret = ibv_cmd_modify_qp(qp, attr, attr_mask, &cmd, sizeof(cmd));
+	ret = ibv_cmd_modify_qp_ex(qp, attr, attr_mask, &cmd_ex.ibv_cmd,
+				   sizeof(cmd_ex), &resp_ex.ibv_resp,
+				   sizeof(resp_ex));

 	if (flag) {
 		pthread_spin_unlock(&hr_qp->rq.lock);
@@ -1564,8 +1567,13 @@ static int hns_roce_u_v2_modify_qp(struct ibv_qp *qp, struct ibv_qp_attr *attr,
 	if (ret)
 		return ret;

-	if (attr_mask & IBV_QP_STATE)
+	if (attr_mask & IBV_QP_STATE) {
 		qp->state = attr->qp_state;
+		if (attr->qp_state == IBV_QPS_RTR) {
+			hr_qp->tc_mode = resp_ex.drv_payload.tc_mode;
+			hr_qp->priority = resp_ex.drv_payload.priority;
+		}
+	}

 	if ((attr_mask & IBV_QP_STATE) && attr->qp_state == IBV_QPS_RESET) {
 		if (qp->recv_cq)
@@ -1579,6 +1587,9 @@ static int hns_roce_u_v2_modify_qp(struct ibv_qp *qp, struct ibv_qp_attr *attr,
 		hns_roce_init_qp_indices(to_hr_qp(qp));
 	}

+	if (hr_qp->tc_mode == HNS_ROCE_TC_MAP_MODE_DSCP)
+		hr_qp->sl = hr_qp->priority;
+
 	record_qp_attr(qp, attr, attr_mask);

 	return ret;
diff --git a/providers/hns/hns_roce_u_verbs.c b/providers/hns/hns_roce_u_verbs.c
index cff9d1d..3b7a67d 100644
--- a/providers/hns/hns_roce_u_verbs.c
+++ b/providers/hns/hns_roce_u_verbs.c
@@ -1449,7 +1449,7 @@ static int get_tclass(struct ibv_context *context, struct ibv_ah_attr *attr,
 struct ibv_ah *hns_roce_u_create_ah(struct ibv_pd *pd, struct ibv_ah_attr *attr)
 {
 	struct hns_roce_device *hr_dev = to_hr_dev(pd->context->device);
-	struct ib_uverbs_create_ah_resp resp = {};
+	struct hns_roce_create_ah_resp resp = {};
 	struct hns_roce_ah *ah;

 	/* HIP08 don't support create ah */
@@ -1477,12 +1477,15 @@ struct ibv_ah *hns_roce_u_create_ah(struct ibv_pd *pd, struct ibv_ah_attr *attr)
 		memcpy(ah->av.dgid, attr->grh.dgid.raw, ARRAY_SIZE(ah->av.dgid));
 	}

-	if (ibv_cmd_create_ah(pd, &ah->ibv_ah, attr, &resp, sizeof(resp)))
+	if (ibv_cmd_create_ah(pd, &ah->ibv_ah, attr, &resp.ibv_resp, sizeof(resp)))
 		goto err;

 	if (ibv_resolve_eth_l2_from_gid(pd->context, attr, ah->av.mac, NULL))
 		goto err;

+	if (resp.tc_mode == HNS_ROCE_TC_MAP_MODE_DSCP)
+		ah->av.sl = resp.priority;
+
 	ah->av.udp_sport = get_ah_udp_sport(attr);

 	return &ah->ibv_ah;
--
2.30.0

