From 3f2ada89f3a277625390bf6789ccd4e7aba08743 Mon Sep 17 00:00:00 2001
From: Lennart Poettering <lennart@poettering.net>
Date: Thu, 24 Mar 2022 13:50:50 +0100
Subject: [PATCH] errno-util: add ERRNO_IS_DEVICE_ABSENT() macro
 
Inspired by: https://github.com/systemd/systemd/pull/22717#discussion_r834254495
 
Reference:https://github.com/systemd/systemd/commit/3f2ada89f3a277625390bf6789ccd4e7aba08743
Conflict:discard change on homework-luks.c
 
---
 src/basic/errno-util.h        | 10 +++++++++-
 src/rfkill/rfkill.c           |  2 +-
 src/udev/udev-builtin-btrfs.c |  3 ++-
 3 files changed, 12 insertions(+), 3 deletions(-)
 
diff --git a/src/basic/errno-util.h b/src/basic/errno-util.h
index 09abf0b7512d..648de50eb497 100644
--- a/src/basic/errno-util.h
+++ b/src/basic/errno-util.h
@@ -138,10 +138,18 @@ static inline bool ERRNO_IS_PRIVILEGE(int r) {
                       EPERM);
 }
 
-/* Three difference errors for "not enough disk space" */
+/* Three different errors for "not enough disk space" */
 static inline bool ERRNO_IS_DISK_SPACE(int r) {
         return IN_SET(abs(r),
                       ENOSPC,
                       EDQUOT,
                       EFBIG);
 }
+
+/* Three different errors for "this device does not quite exist" */
+static inline bool ERRNO_IS_DEVICE_ABSENT(int r) {
+        return IN_SET(abs(r),
+                      ENODEV,
+                      ENXIO,
+                      ENOENT);
+}
diff --git a/src/rfkill/rfkill.c b/src/rfkill/rfkill.c
index 656afa06ac8b..a833771d97f2 100644
--- a/src/rfkill/rfkill.c
+++ b/src/rfkill/rfkill.c
@@ -80,7 +80,7 @@ static int find_device(
 
         r = sd_device_new_from_subsystem_sysname(&device, "rfkill", sysname);
         if (r < 0)
-                return log_full_errno(IN_SET(r, -ENOENT, -ENXIO, -ENODEV) ? LOG_DEBUG : LOG_ERR, r,
+                return log_full_errno(ERRNO_IS_DEVICE_ABSENT(r) ? LOG_DEBUG : LOG_ERR, r,
                                       "Failed to open device '%s': %m", sysname);
 
         r = sd_device_get_sysattr_value(device, "name", &name);
diff --git a/src/udev/udev-builtin-btrfs.c b/src/udev/udev-builtin-btrfs.c
index a0093cb42347..f9d4f1dd4ef4 100644
--- a/src/udev/udev-builtin-btrfs.c
+++ b/src/udev/udev-builtin-btrfs.c
@@ -6,6 +6,7 @@
 #include <sys/ioctl.h>
 
 #include "device-util.h"
+#include "errno-util.h"
 #include "fd-util.h"
 #include "string-util.h"
 #include "strxcpyx.h"
@@ -22,7 +23,7 @@ static int builtin_btrfs(sd_device *dev, sd_netlink **rtnl, int argc, char *argv
 
         fd = open("/dev/btrfs-control", O_RDWR|O_CLOEXEC);
         if (fd < 0) {
-                if (IN_SET(errno, ENOENT, ENXIO, ENODEV)) {
+                if (ERRNO_IS_DEVICE_ABSENT(errno)) {
                         /* Driver not installed? Then we aren't ready. This is useful in initrds that lack
                          * btrfs.ko. After the host transition (where btrfs.ko will hopefully become
                          * available) the device can be retriggered and will then be considered ready. */
 
