From 9b1d5d040d82db567c9ab0ea2b271b6d12e8969f Mon Sep 17 00:00:00 2001
From: Nicolas Melot <nicolas.melot@ericsson.com>
Date: Sun, 1 Aug 2021 19:20:58 +0200
Subject: [PATCH] Forward value of sector_size instead of its address in
 blkdev_get_physector_size

---
 lib/blkdev.c | 4 +++-
 1 file changed, 3 insertions(+), 1 deletion(-)

diff --git a/lib/blkdev.c b/lib/blkdev.c
index c22853d..2d02fb8 100644
--- a/lib/blkdev.c
+++ b/lib/blkdev.c
@@ -222,8 +222,10 @@ int blkdev_get_sector_size(int fd __attribute__((__unused__)), int *sector_size)
 #ifdef BLKPBSZGET
 int blkdev_get_physector_size(int fd, int *sector_size)
 {
-	if (ioctl(fd, BLKPBSZGET, &sector_size) >= 0)
+	if (ioctl(fd, BLKPBSZGET, sector_size) >= 0)
+    {
 		return 0;
+    }
 	return -1;
 }
 #else
-- 
1.8.3.1

